
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***02*,;PACKAGE:0402,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***03*,;PACKAGE:0603,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***05*,;PACKAGE:1005,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***08*,;PACKAGE:0808,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***0D*,;PACKAGE:0404,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***15*,;PACKAGE:1005,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***18*,;PACKAGE:1608,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***1U*,;PACKAGE:0610,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***21*,;PACKAGE:2012,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***22*,;PACKAGE:2828,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***31*,;PACKAGE:3216,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***32*,;PACKAGE:3225,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***42*,;PACKAGE:4520,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***43*,;PACKAGE:4532,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:***55*,;PACKAGE:5750,;

[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********0E*,;TAIATU:2.5V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********0G*,;TAIATU:4V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********0J*,;TAIATU:6.3V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********1A*,;TAIATU:10V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********1C*,;TAIATU:16V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********1E*,;TAIATU:25V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********1H*,;TAIATU:50V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********1J*,;TAIATU:63V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********1K*,;TAIATU:80V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********2A*,;TAIATU:100V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********2D*,;TAIATU:200V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********2E*,;TAIATU:250V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********2W*,;TAIATU:450V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********2H*,;TAIATU:500V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********2J*,;TAIATU:630V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********3A*,;TAIATU:1000V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********3D*,;TAIATU:2000V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********3F*,;TAIATU:3150V,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:********YA*,;TAIATU:35000V,;

[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********1R0*,;VALUE:1P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********2R0*,;VALUE:2P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********3R0*,;VALUE:3P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********4R0*,;VALUE:4P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********5R0*,;VALUE:5P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********6R0*,;VALUE:6P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********7R0*,;VALUE:7P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********8R0*,;VALUE:8P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********9R0*,;VALUE:9P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********100*,;VALUE:10P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********120*,;VALUE:12P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********150*,;VALUE:15P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********180*,;VALUE:18P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********220*,;VALUE:22P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********270*,;VALUE:27P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********330*,;VALUE:33P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********390*,;VALUE:39P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********470*,;VALUE:47P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********560*,;VALUE:56P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********680*,;VALUE:68P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********820*,;VALUE:82P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********101*,;VALUE:100P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********121*,;VALUE:120P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********151*,;VALUE:150P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********181*,;VALUE:180P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********221*,;VALUE:220P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********271*,;VALUE:270P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********331*,;VALUE:330P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********391*,;VALUE:390P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********471*,;VALUE:470P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********561*,;VALUE:560P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********681*,;VALUE:680P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********821*,;VALUE:820P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********102*,;VALUE:1000P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********122*,;VALUE:1200P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********152*,;VALUE:1500P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********182*,;VALUE:1800P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********222*,;VALUE:2200P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********272*,;VALUE:2700P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********332*,;VALUE:3300P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********472*,;VALUE:4700P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********682*,;VALUE:6800P,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********103*,;VALUE:0.01U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********153*,;VALUE:0.015U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********223*,;VALUE:0.022U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********333*,;VALUE:0.033U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********473*,;VALUE:0.047U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********683*,;VALUE:0.068U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********104*,;VALUE:0.1U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********154*,;VALUE:0.15U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********224*,;VALUE:0.22U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********334*,;VALUE:0.33U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********474*,;VALUE:0.47U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********684*,;VALUE:0.68U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********105*,;VALUE:1U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********155*,;VALUE:1.5U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********225*,;VALUE:2.2U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********335*,;VALUE:3.3U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********475*,;VALUE:4.7U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********106*,;VALUE:10U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********226*,;VALUE:22U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********476*,;VALUE:47U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********107*,;VALUE:100U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********227*,;VALUE:220U,;
[>]TYPE:Ref,RTYPE:C,MAKER:MURATA,<NAST>MODEL:**********477*,;VALUE:470U,;

